# STANDARD ST. XX

RECOMMENDATIONS ON DIGITAL THREE-DIMENSIONAL (3D) MODELS AND 3D IMAGES

Revised proposal considering the discussions at CWS/9.

## INTRODUCTION

 This Standard provides recommendations for Intellectual Property Offices (IPOs) and other interested parties that manage, store, process, exchange or disseminate IP data using 3D models and 3D images.

 This Standard has the following objectives:

1. determination of formats that are available, compatible or interoperable with different software used by applicants in order to facilitate their efforts to prepare application materials before filing;
2. reducing the time of IP application processing by IPOs;
3. facilitating IP application filing to different IPOs due to adoption of recommended formats among IPOs;
4. harmonization of requirements for data exchange on subjects for IP rights protection with digital 3D visual representations among IPOs and other organizations; and
5. set of requirements for the publication of information on subjects for IP rights protection with digital 3D visual representations.

DEFINITIONS

 For the purposes of this Standard, unless otherwise specified:

1. 3D model – An electronic file that is created by specialized software, for mathematically representing the surface of an object’s visual representation in three dimensions;
2. 3D Images – Digital images that represent objects displayed in three dimensions such as 3D photos and stereoscopy;
3. CAD – computer aided design;
4. 3D PDF – a PDF document that contains 3D models;
5. IGES – Initial Graphics Exchange Specification;
6. OBJ – An open geometry vertex file format used for CAD and 3D printing;
7. CDX/MOL – A text-based chemical file format that describes molecules and chemical reactions;
8. PDF – The Portable Document Format is a file format developed by Adobe;
9. Raster image – An image that is composed of a map of points (pixels), referred to as a bitmap. Typical file formats for raster images include JPEG, TIFF, PNG and BMP;
10. STL – Standard Tessellation Language – a file format native to the stereolithography CAD software created by 3D Systems;
11. STEP – Standard for the Exchange of Product model data – an open ISO Standard which can represent 3D objects in Computer-aided design (CAD) and related information;
12. U3D – Universal 3D (U3D) is a compressed file format standard for 3D computer graphics data;
13. Vector graphics – An image file that is composed of shapes formed of mathematical formulas and coordinates on a 2D plane. As opposed to raster images, vector graphics have the property of scaling infinitely without any degradation of quality; and
14. X3D – Successor of VRML, an Open ISO Standard XML format.

REFERENCES

 The following WIPO Standards and other documents are relevant to the present Standard:

|  |  |
| --- | --- |
| WIPO Standard ST.9 | Bibliographic data on and relating to patents and SPCs |
| WIPO Standard ST.10 | Published patent documents |
| WIPO Standard ST.60 | Bibliographic data relating to marks |
| WIPO Standard ST.63 | Content and layout of trademark gazettes |
| WIPO Standard ST.67 | Electronic management of the figurative elements of trademarks |
| WIPO Standard ST.80 | Bibliographic data relating to industrial designs |
| WIPO Standard ST.81 | Content and layout of industrial designs gazettes |
| WIPO Standard ST.88 | Electronic representation of industrial designs |
| WIPO Standard ST.96 | Processing of Industrial Property information using XML |
| ISO Standard 10303 | Product data representation and exchange standard |

GENERAL RECOMMENDATIONS

 An application for IP protection may contain a 3D visual representation of an object in the form of a digital 3D model or 3D image in accordance with the requirements of the IPO receiving the application. Applicants can be encouraged to provide a 3D visual representation of the object as supplementary material to the application or as the main visual representation of the object, if specified by the requirements of the receiving IPO.

 Formats and other characteristics of the received image files (e.g., file size) accepted by each IPO should be according to the recommendations of this Standard.

 If an IPO has previously established its preferred image formats and other characteristics, it is recommended that the IPO announce in its official publications at regular intervals and/or on its websites, the image formats, sizes and other specific characteristics that are acceptable in application filings.

RECOMMENDATIONS FOR 3D MODELS AND 3D IMAGES FORMATS AND FILE SIZE

 The following recommendations apply to providing application materials for the indicated type of IP rights.

### Patent for invention or utility model

 3D visual representation of an invention or utility model should preferably be formatted as at least one of the formats: STEP, IGES, U3D, OBJ or STL. Maximum file size should not exceed 50 MB. If required, at an applicant’s request the receiving IPO can accept files larger than the said maximum.

 For chemical structures that are included in patent applications, 3D visual representation should preferably be formatted as CDX or MOL. Maximum file size should not exceed 50 MB.

### Industrial design

 3D visual representation of an industrial design should preferably be formatted as at least one of the formats: STEP, IGES, U3D, OBJ or STL. Maximum file size should not exceed 50 MB. If required, at an applicant’s request the receiving IPO can accept files larger than the said maximum.

### Trademark

 3D visual representation of a trademark should preferably be formatted as at least one of the formats: STEP, IGES, U3D, OBJ or STL. Maximum file size should not exceed 50 MB. If required, at an applicant’s request the receiving IPO can accept files larger than the said maximum.

### Integrated circuit topography

 3D visual representation of an integrated circuit topography should preferably be formatted as at least one of the formats: STEP, IGES, U3D, OBJ or STL. Maximum file size should not exceed 50 MB. If required, at an applicant’s request the receiving IPO can accept files larger than the said maximum.

PROCEDURAL RECOMMENDATIONS FOR FILING AND PROCESSING OF 3D MODELS AND 3D IMAGES

 If an IPO converts a 3D model or 3D image from formats originally submitted by applicants to formats other than recommended above, or transforms from one storage format to another (e.g. STEP to STL), it is recommended that the IPO retain the original format as well as the transformed format for archival purposes.

 If an IPO receives a 3D model or 3D image as the only visual representation of an object in an application for IP right protection and needs 2D images, it is recommended to make 2D views of the 3D model in order to ensure compatibility with the IPO’s internal systems and processes where only 2D images of objects are required.

1. For patent applications for inventions or utility models, it is recommended to make seven 2D views of the 3D model, i.e., front, rear, right, left, top, bottom, and perspective views, in an electronic format corresponding to the requirements established by the IPO for 2D images of inventions or utility models.
2. For industrial design applications, it is recommended to make six 2D views of the 3D model, i.e., front, back, left, right, top, and bottom views, in an electronic format corresponding to the requirements established by the IPO for 2D images of industrial designs.
3. For trademark applications, it is recommended to make one 2D view of the 3D model, i.e., front view, in an electronic format corresponding to the requirements established by the IPO for 2D images of figurative trademarks.

 It is recommended that an IPO define a set of guidelines and procedures for converting models and images from 3D to 2D formats.

RECOMMENDATIONS FOR DATA EXCHANGE

 When IPOs exchange 3D model and/or 3D image data, file formats can be converted from the original formats, if such is established by an IPO. The conversion or transformation from the original file formats should be conducted in accordance with the guidelines and procedures established by the IPOs involved. The following additional requirements are recommended when exchanging application data for the indicated type of IP rights.

### Patents for inventions or utility models

 It is recommended that IPOs and other organizations comply with the following requirements when exchanging 3D models and/or 3D images data incorporated in patent documents:

* + At least one of the file formats: U3D, OBJ or STL, STEP, IGES; and
	+ Maximum file size: 50 MB.

 For the chemical structures in the patent application, it is recommended that IPOs and other organizations comply with the following requirements when exchanging 3D models and/or 3D images:

* + At least one of the file formats: MOL, CDX

### Industrial designs

 It is recommended that IPOs and other organizations comply with the following requirements when exchanging 3D models and/or 3D images incorporated in industrial design applications:

* + At least one of the file formats: U3D, OBJ or STL, STEP, IGES; and
	+ Maximum file size: 50 MB.

### Trademarks

 It is recommended that IPOs and other organizations comply with the following requirements when exchanging 3D models and/or 3D images incorporated in trademark applications:

* + At least one of the file formats: U3D, OBJ or STL, STEP, IGES; and
	+ Maximum file size: 50 MB.

RECOMMENDATIONS FOR ELECTRONIC PUBLICATION AND ONLINE DISPLAY

 It is recommended that an electronic publication of an object in an IP application or IP right include 3D model and/or 3D image files received by the IPO in the list of published documents relating to the IP application or IP right.

 Formats of published 3D files can be converted from the original formats, if desired by the IPO. Any conversions or transformations should be conducted in accordance with the guidelines and procedures established by the IPO.

 For online display of 3D visual representation of an object, the following requirements are recommended:

* + At least one of the file formats: U3D, OBJ or STL, STEP, IGES, MOL, CDX: OBJ or STL; and
	+ Maximum file size: 50 MB.

 For electronic publication of 3D visual representations of an object in PDF format, it is recommended to create files in 3D PDF embedding the 3D models and/or 3D images in one of the 3D file formats recommended under this Standard. If the original 3D model cannot be embedded in 3D PDF in its original format, then it is recommended to convert the 3D model to one of the 3D file formats recommended under this Standard, or to embed 2D image(s) of the object, preferably as received from the applicant, or as converted by the IPO from 3D formats submitted by the applicant.

 Paper publication should contain a 2D visual representation of a 3D object and/or a link to the 3D object online.

RECOMMENDATIONS FOR PARTIAL CLAIMING, PARTIAL DESIGN, PORTION DESIGN

 It is recommended that appropriate depiction of partial claiming of design, partial design, or portion design should be feasible in a relevant 3D format, and disclaimed features in designs should be readily recognizable and understandable.

 The depictions of partial claiming of design, partial design, and portion design featured in relevant 3D format should be robustly maintained during processing of applications with 3D models or 3D images, e.g., when publishing the applications.

[End of ST.XX]

[End of Annex and document]